**PUBLIC NOTICE**

**BUNN PARK COMBINED SEWER OVERFLOW IMPROVEMENTS**

The Sangamon County Water Reclamation District is making improvements to the sewers in the Bunn Park combined sewer area to convey more wet weather flow to the Sugar Creek sewage treatment plant as required by the approved CSO Long-Term Control Plan and the current National Pollutant Discharge Elimination System (NPDES) Permit requirements. The project includes the following:

* Constructing new 54-inch diameter sewer on South 15th Street, from East Oberlin to East Lenox Streets and connecting to existing sewers with set over reinforced concrete structures.
* Reconnecting six existing sewer service connections from the existing 18-inch diameter sewer on South 15th Street to the proposed 54-inch diameter sewer and installing over-head sewer systems inside three of the residences.
* Making modifications to existing diversion structure near the #5 Tee Box on the Bunn Park Golf Course, adjacent to Fox Bridge Road.
* Constructing new 42-inch diameter sewer on East Cornell Avenue at the intersection of South 16th Street and a new reinforced concrete structure to join the 42-inch sewer to an existing 66-inch diameter sewer.
* Removing and replacing 66-inch diameter reinforced concrete combined sewer pipe and laying new 24-inch diameter storm sewer pipe on East Cornell Avenue.
* Constructing new storm sewer to disconnect street inlets from the combined sewer.

The improvements are to be constructed around the Bunn Park golf course area, in Springfield, Illinois. Funding for this project is provided by a low interest loan from the Illinois Environmental Protection Agency’s Water Pollution Control Loan Program (WPCLP). The WPCLP is funded by both State and Federal sources. The $2,768,768.08 loan has an interest rate of 1.11% and will be repaid over 20 years. For more information contact the Sangamon County Water Reclamation District.

[](https://www2.illinois.gov/epa/) Logo of the United States Environmental Protection Agency 